The Simplest Version: 
Micro:bit’s LEDs Screen & Buzzer, MQ2 = P0
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2nd Version: 
Micro:bit’s LEDs Screen & Buzzer, MQ2 = P0, 
LED lightbulb (Flashing) = P1



3rd Version: 
Micro:bit’s LEDs Screen & Buzzer, MQ2 = P0, 
[bookmark: _GoBack]LED lightbulb (Flashing) = P1, Water Pump (With relay) = P2
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